|  |  |  |  |
| --- | --- | --- | --- |
| **Bid Bulletin Ref. No.** | **Specific Page/Section in the Bidding Docs.** | **Query/Issue** | **BAC Response/Clarification** |
| BB1-1 | Page 10Item No. 2Section IInvitation to Bid | Delivery of the Goods is required within thirty (30) calendar days upon receipt of Notice to Proceed. | Delivery of the Goods is required within forty five (45) calendar days for NCR and Central Office (CO), while sixty (60) calendar days for Field offices upon receipt of Notice to Proceed (NTP). |
| BB1-2 | Page 51ITB Clause5.4Section IIIBid Data Sheet | The bidder’s SLCC similar to the contract to be bid should have been completed within two (2) years prior to the deadline for the submission and receipt of bids.The bidder’s SLCC is based on by lot or the total project cost. | From two (2) years to three (3) years prior to the deadline for the submission and receipt of bids.The Bidder must have completed, within the period specified in the Invitation to Bid and ITB Clause 12.1(a)(ii), a single contract that is similar to this Project, equivalent to at least fifty percent (50%) of the ABC**per Lot**. |
| BB1-3 | Page 85Section VISchedule of Requirements | Under Delivered, Weeks/MonthsWithin thirty (30) days upon receipt of Notice to Proceed | Within forty five (45) calendar days for NCR and CO while sixty (60) calendar days for Field Offices upon receipt of NTP. |
| BB1-4 | Page 86Section VISchedule of Requirements | Delivery Sites and Contact PersonsProject Site PSA, Centris 1Within 30 days upon issuance of NTP | Within forty five (45) days upon issuance of NTP |
| BB1-5 | Page 86Section VISchedule of Requirements | Under Delivery Sites and Contact PersonsDelivery SitePSA Central and Field OfficesSee **Annex A** for the Hardware Distribution list to PSA Field Offices nationwide | See **Attachment A** for the revised Hardware Distribution list to PSA Field Offices nationwide |
| BB1-6 | Page 86Section VISchedule of Requirements | Under Delivery Sites and Contact PersonsDelivery SitePSA Central and Field OfficesWithin 30 days upon issuance of NTP | Within forty five (45) calendar days for NCR and CO while sixty (60) calendar days for Field offices upon issuance of NTP. |
| BB1-7 | Page 90Section VIITechnical Specifications(8.0’” Android Tablet with 32 GB SD Card and Flip Cover) | Under *Accessories Included*with Generic Cover/Tablet Case | Revised to:with Cover/Tablet Case |
| BB1-8 | Page 90Section VIITechnical Specifications(8.0’” Android Tablet with 32 GB SD Card and Flip Cover) | Under *Warranty*One (1) year on on-site nationwide support; | Revised to:One (1) year on-site support within Metro Manila and carry-in for outside Metro Manila; |
| BB1-9 | Page 90Section VIITechnical Specifications(8.0’” Android Tablet with 32 GB SD Card and Flip Cover)Page 92 and 93(Desktop with MS Office and OS andDesktop with MS Office with MS Access and OS)Page 96(GIS Ready Desktop) | Under *Additional Requirement*“Bidder must be authorizedreseller of the brand beingoffered.” Is a back to back certificate acceptable - Certificate issued by manufacturer to distributor and distributor to authorized reseller? | Yes, a back to back certificate is acceptable – Certificate issued by manufacturer to distributor and distributor to authorized reseller.A list of authorized service centers should be provided. |
| BB1-10 | Page 91 and 92Section VIITechnical Specifications(Desktop with MS Office and OS andDesktop with MS Office with MS Access and OS) | Under *Standard I/O Ports*,1 USB 2.0 (fast charging);The bidder inquired if the USB 2.0 needs to be fast charging.1 DisplayPort™ 1.2; 1 HDMI; 1 serial; 1 USB Type-C™; 1 VGA | Revised to:1 USB 2.01 VGA or 1 HDMI |
| BB1-11 | Page 91 and 93Section VIITechnical Specifications(Desktop with MS Office and OS andDesktop with MS Office with MS Access and OS) | Under *Audio-in/out jacks*,HD audio Combo Microphone/Headphone Jack, with Realtek ALC221, Line-out and Line-in rear port (3.5mm), Standard internal speaker | Revised to:Integrated high definition audio |
| BB1-12 | Page 91 and 93Section VIITechnical Specifications(Desktop with MS Office and OS andDesktop with MS Office with MS Access and OS) | Under *Expansions slots*2 full-height PCIe x16, one wired as x4 | Revised to:2 full-height PCIe x16, one wired as x4 (using x16 connector) |
| BB1-13 | Page 91 and 93Section VIITechnical Specifications(Desktop with MS Office and OS andDesktop with MS Office with MS Access and OS) | Under *Additional Software*Kaspersky Anti-Virus with three (3) years subscription (pre-installed and activated) | Revised to:Kaspersky Antivirus Enterprise Edition with three (3) years subscription (installed and activated) |
| BB1-14 | Page 92 and 93Section VIITechnical Specifications(Desktop with MS Office and OS andDesktop with MS Office with MS Access and OS) | Under *Warranty*Three (3) years on on-site nationwide support; | Revised to:Three (3) years on-site support; |
| BB1-15 | Page 93 and 96Section VIITechnical Specifications(UPS 1000VA for Desktop and UPS 1000VA for GIS Desktop) | Under *Input;*Voltage: 120VAC or 230VAC Under Output;Output Waveform: 50Hz or 60Hz +/-1 Hz | Revised to:Voltage: 120VAC - 230VACOutput Waveform: Step wave or Sine wave |
| BB1-16 | Page 94 and 96Section VIITechnical Specifications(UPS 1000VA for Desktop and UPS 1000VA for GIS Desktop) | Under *Battery;*Output Waveform: 12V/7AH x 2pcUnder *Interface;*RJ 45 and USB | Revised to:Output Waveform: Same capacity or higherPreferably USB only |
| BB1-17 | Page 94 Section VIITechnical Specifications(UPS 1000VA for Desktop) | Under *Warranty;*Two (2) years on on-site nationwide support; | Revised to:Two (2) years on on-site support; |
| BB1-18 | Page 95Section VIITechnical Specifications(GIS Ready Desktop) | Under *Additional Software;*Endpoint solution for business (1 Yr subscription) - must be compatible with the existing PSA antivirusWhat is the existing PSA antivirus? | Kaspersky Antivirus Enterprise Edition  |
| BB1-19 | Page 97 Section VIITechnical Specifications(4-Bay NAS with 2 Storage Devices 8 TB) | with two (2) x 8 TB HDD NAS Drives (7200rpm, 256 MB cache, compatible with NAS, installed and preconfigured with Raid 10) | Revised to:with two (2) x 8 TB HDD NAS Drives (7200rpm, 256 MB cache, compatible with NAS, installed and preconfigured with **Raid 1,0**) |
| BB1-20 | Page 98 Section VIITechnical Specifications(12-Bay NAS with 9 Storage Devices 4 TB) | Under *External Ports;*Wireless Support (dongle) | Optional Wireless Support (dongle) |
| BB1-21 | Page 99Section VIITechnical Specifications(12-Bay NAS with 9 Storage Devices 4 TB) | Delivery: Nationwide Shipment | Revised to:Delivery: Central Office |
| BB1-22 | Page 99Section VIITechnical Specifications(12-Bay NAS with 9 Storage Devices 4 TB) | Under *Additional Requirement*Bidder must be authorized reseller of the brand being offered. | Bidder must be authorized reseller of the brand being offered or a Back-to-Back Certificate (Manufacturer to Distributor, Distributor to Reseller) |
| BB1-23 | Page 99 Section VIITechnical Specifications(Rack-mounted Tower Server) | Under *Video Controller;*at least 16bit color maximum resolution of 1920 x1200 Integrated Matrox G200 Video standard with 16MB flash, 256MB DDRUnder *Expansion Slots*;Expansion Slots: 9 Slots on-board PCI Express slotBidder requested for 6 slots only.Under *Power Supply;*Dual Power Supply hot-pluggable upgradable to four (4) | Revised to:Matrox G200 Video to be replaced with Manufacturers’ standard 6 Slots on-board PCI Express slotDual Power Supply hot-pluggable upgradable to two (2) |
| BB1-24 | Section VIITechnical Specifications(UPS for Server) | Bidders asked regarding installation requirements | The winning bidder must provide single-line diagram. |
| BB1-25 | Page 101Section VIITechnical Specifications(UPS for Server) | Under *Backup Runtime/Batteries;**Replacement Battery*: GXT4-240VBATKIT*Extended Run Options*: Up to 6 External Battery Cabinets (P/N: GXT4-240VBATT) | Revised to:*Replacement Battery*: Battery Pack*Extended Run Options*: Up to 6 External Battery Cabinets |
| BB1-26 | Page 102Section VIITechnical Specifications(UPS for Server) | Under *Communications and Management**Available IntelliSlot Quantity*:1 (SNMP, 485, Relay interface cards available)*Power Management Software*: Multilink Shutdown Software (Installation CD included) | Revised to:*Available IntelliSlot Quantity*: 1 (SNMP and Web Management capability or equivalent)*Power Management Software*:Multilink Shutdown Software or equivalent |
| BB1-27 | Page 9Item 1, Section IInvitation to Bid |  | should be;1. The Philippine Statistics Authority (PSA), through the ***2018***General Appropriation Act, intends to apply the sum… |
| BB1-28 |  | For items to be delivered in the Regions/Provinces, how is the acceptance? | There will be assigned focal persons who will sign or receive the Delivery Receipts (DR). |
| BB1-29 |  | Will you allow partial payment for partial delivery?What are the required attachments for the billing? | Yes.The required attachments are the Delivery Receipts (DR) and Inspection Reports duly signed by the authorized focal persons. Sales Invoice per billing with the corresponding attachments will be addressed to the PSA Central Office.  |